It is important to follow the reset procedure below when resetting alarms with SigmaLogic. Otherwise the alarms might not reset properly.

Step 1) Release all active AOI’s

Step 2) Toggle MAS\_Yaskawa (The AOI will stop the servo)

Step 3) Toggle MSF\_Yaskawa (This AOI will disable the servo)

Step 4) Toggle MAFR\_Yaskawa (This AOI will reset the fault)

Then you will be able to re-enable the servo and continue. This procedure is also covered in the SigmaLogic QuickStart Control video.